Use serial port assistant 
1 Open the serial port assistant and set the parameters
1 Read the voltage of channel 1   = 4.01v
2 Read the voltage of channel 2   = 3.99V
   (1)modify the register 
   (2)   recalculate the CRC
3 Follow step 2 for other channels   Channel 3 = 0A


