7 segment display driver for JY-MCU module based on TM1650 chip
Copyright (c) 2015 Anatoli Arkhipenko

Changelog:
	v1.0.0:
		2015-02-24 - Initial release 
 
	v1.0.1:  
		2015-04-27 - Added support of program memery (PROGMEM) to store the ASCII to Segment Code table

	v1.0.2
		2015-08-08 - Added check if panel is connected during init. All calls will be disabled is panel was not connected during init.

	v1.1.0:
		2015-12-20 - Code clean up. Moved to a single header file. Added Gradual brightness method