;
; Copyright 2015 Arduino LLC (http://www.arduino.cc/)
;
; Developed by Zach Eveland, Blacklabel Development, Inc.
;
; Arduino is free software; you can redistribute it and/or modify
; it under the terms of the GNU General Public License as published by
; the Free Software Foundation; either version 2 of the License, or
; (at your option) any later version.
;
; This program is distributed in the hope that it will be useful,
; but WITHOUT ANY WARRANTY; without even the implied warranty of
; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
; GNU General Public License for more details.
;
; You should have received a copy of the GNU General Public License
; along with this program; if not, write to the Free Software
; Foundation, Inc., 51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
;
; As a special exception, you may use this file as part of a free software
; library without restriction.  Specifically, if other files instantiate
; templates or use macros or inline functions from this file, or you compile
; this file and link it with other files to produce an executable, this
; file does not by itself cause the resulting executable to be covered by
; the GNU General Public License.  This exception does not however
; invalidate any other reasons why the executable file might be covered by
; the GNU General Public License.
;

[Strings]
DriverPackageDisplayName="Arduino USB Driver"
ManufacturerName="Arduino LLC (www.arduino.cc)"
ServiceName="USB RS-232 Emulation Driver"
bossa.name="Bossa Program Port"
due.programming_port.name="Arduino Due Programming Port"
due.sketch.name="Arduino Due"
esplora.bootloader.name="Arduino Esplora bootloader"
esplora.sketch.name="Arduino Esplora"
leonardo.bootloader.name="Arduino Leonardo bootloader"
leonardo.sketch.name="Arduino Leonardo"
lilypadUSB.bootloader.name="Arduino LilyPad USB bootloader"
lilypadUSB.sketch.name="Arduino LilyPad USB"
mega2560.name="Arduino Mega 2560"
mega2560rev3.name="Arduino Mega 2560"
megaADK.name="Arduino Mega ADK"
megaADKrev3.name="Arduino Mega ADK"
micro.bootloader.name="Arduino Micro bootloader"
micro.sketch.name="Arduino Micro"
mkr1000.sketch.name="Arduino MKR1000"
mkr1000.bootloader.name="Arduino MKR1000 bootloader"
robotControl.bootloader.name="Arduino Robot Control bootloader"
robotControl.sketch.name="Arduino Robot"
robotMotor.bootloader.name="Arduino Robot Motor bootloader"
robotMotor.sketch.name="Arduino Robot"
uno.name="Arduino Uno"
unoR3.name="Arduino Uno"
usbserial.name="Arduino USB Serial Light Adapter"
yun.bootloader.name="Arduino Yun bootloader"
yun.sketch.name="Arduino Yun"
zero.edbg.name="Atmel Corp. EDBG CMSIS-DAP"
zero.sketch.name="Arduino Zero"
zero.bootloader.name="Arduino Zero bootloader"
sme_fox.sketch.name="SmartEverything Fox"
sme_fox.bootloader.name="SmartEverything Fox bootloader"

[DefaultInstall]
CopyINF=arduino.inf

[Version]
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Signature="$Windows NT$"
Provider=%ManufacturerName%
DriverPackageDisplayName=%DriverPackageDisplayName%
CatalogFile=arduino.cat
DriverVer=11/24/2015,1.2.3.0

[Manufacturer]
%ManufacturerName%=DeviceList, NTamd64, NTia64

[DestinationDirs]
FakeModemCopyFileSection=12
DefaultDestDir=12

[DeviceList]
%bossa.name%=DriverInstall, USB\VID_03EB&PID_6124
%due.programming_port.name%=DriverInstall, USB\VID_2341&PID_003D
%due.sketch.name%=DriverInstall, USB\VID_2341&PID_003E&MI_00
%esplora.bootloader.name%=DriverInstall, USB\VID_2341&PID_003C
%esplora.sketch.name%=DriverInstall, USB\VID_2341&PID_803C&MI_00
%leonardo.bootloader.name%=DriverInstall, USB\VID_2341&PID_0036
%leonardo.sketch.name%=DriverInstall, USB\VID_2341&PID_8036&MI_00
%lilypadUSB.bootloader.name%=DriverInstall, USB\VID_1B4F&PID_9207
%lilypadUSB.sketch.name%=DriverInstall, USB\VID_1B4F&PID_9208&MI_00
%mega2560rev3.name%=DriverInstall, USB\VID_2341&PID_0042
%mega2560.name%=DriverInstall, USB\VID_2341&PID_0010
%megaADK.name%=DriverInstall, USB\VID_2341&PID_003F
%megaADKrev3.name%=DriverInstall, USB\VID_2341&PID_0044
%micro.bootloader.name%=DriverInstall, USB\VID_2341&PID_0037
%micro.sketch.name%=DriverInstall, USB\VID_2341&PID_8037&MI_00
%mkr1000.sketch.name%=DriverInstall, USB\VID_2341&PID_804E&MI_00
%mkr1000.bootloader.name%=DriverInstall, USB\VID_2341&PID_004E
%robotControl.bootloader.name%=DriverInstall, USB\VID_2341&PID_0038
%robotControl.sketch.name%=DriverInstall, USB\VID_2341&PID_8038&MI_00
%robotMotor.bootloader.name%=DriverInstall, USB\VID_2341&PID_0039
%robotMotor.sketch.name%=DriverInstall, USB\VID_2341&PID_8039&MI_00
%uno.name%=DriverInstall, USB\VID_2341&PID_0001
%unoR3.name%=DriverInstall, USB\VID_2341&PID_0043
%usbserial.name%=DriverInstall, USB\VID_2341&PID_003B
%yun.bootloader.name%=DriverInstall, USB\VID_2341&PID_0041
%yun.sketch.name%=DriverInstall, USB\VID_2341&PID_8041&MI_00
%zero.edbg.name%=DriverInstall, USB\VID_03EB&PID_2157&MI_01
%zero.sketch.name%=DriverInstall, USB\VID_2341&PID_804D&MI_00
%zero.bootloader.name%=DriverInstall, USB\VID_2341&PID_004D
%sme_fox.sketch.name%=DriverInstall, USB\VID_2341&PID_E002&MI_00
%sme_fox.bootloader.name%=DriverInstall, USB\VID_2341&PID_E001

[DeviceList.NTamd64]
%bossa.name%=DriverInstall, USB\VID_03EB&PID_6124
%due.programming_port.name%=DriverInstall, USB\VID_2341&PID_003D
%due.sketch.name%=DriverInstall, USB\VID_2341&PID_003E&MI_00
%esplora.bootloader.name%=DriverInstall, USB\VID_2341&PID_003C
%esplora.sketch.name%=DriverInstall, USB\VID_2341&PID_803C&MI_00
%leonardo.bootloader.name%=DriverInstall, USB\VID_2341&PID_0036
%leonardo.sketch.name%=DriverInstall, USB\VID_2341&PID_8036&MI_00
%lilypadUSB.bootloader.name%=DriverInstall, USB\VID_1B4F&PID_9207
%lilypadUSB.sketch.name%=DriverInstall, USB\VID_1B4F&PID_9208&MI_00
%mega2560rev3.name%=DriverInstall, USB\VID_2341&PID_0042
%mega2560.name%=DriverInstall, USB\VID_2341&PID_0010
%megaADK.name%=DriverInstall, USB\VID_2341&PID_003F
%megaADKrev3.name%=DriverInstall, USB\VID_2341&PID_0044
%micro.bootloader.name%=DriverInstall, USB\VID_2341&PID_0037
%micro.sketch.name%=DriverInstall, USB\VID_2341&PID_8037&MI_00
%mkr1000.sketch.name%=DriverInstall, USB\VID_2341&PID_804E&MI_00
%mkr1000.bootloader.name%=DriverInstall, USB\VID_2341&PID_004E
%uno.name%=DriverInstall, USB\VID_2341&PID_0001
%unoR3.name%=DriverInstall, USB\VID_2341&PID_0043
%usbserial.name%=DriverInstall, USB\VID_2341&PID_003B
%robotControl.bootloader.name%=DriverInstall, USB\VID_2341&PID_0038
%robotControl.sketch.name%=DriverInstall, USB\VID_2341&PID_8038&MI_00
%robotMotor.bootloader.name%=DriverInstall, USB\VID_2341&PID_0039
%robotMotor.sketch.name%=DriverInstall, USB\VID_2341&PID_8039&MI_00
%yun.bootloader.name%=DriverInstall, USB\VID_2341&PID_0041
%yun.sketch.name%=DriverInstall, USB\VID_2341&PID_8041&MI_00
%zero.edbg.name%=DriverInstall, USB\VID_03EB&PID_2157&MI_01
%zero.sketch.name%=DriverInstall, USB\VID_2341&PID_804D&MI_00
%zero.bootloader.name%=DriverInstall, USB\VID_2341&PID_004D
%sme_fox.sketch.name%=DriverInstall, USB\VID_2341&PID_E002&MI_00
%sme_fox.bootloader.name%=DriverInstall, USB\VID_2341&PID_E001

[DeviceList.NTia64]
%bossa.name%=DriverInstall, USB\VID_03EB&PID_6124
%due.programming_port.name%=DriverInstall, USB\VID_2341&PID_003D
%due.sketch.name%=DriverInstall, USB\VID_2341&PID_003E&MI_00
%esplora.bootloader.name%=DriverInstall, USB\VID_2341&PID_003C
%esplora.sketch.name%=DriverInstall, USB\VID_2341&PID_803C&MI_00
%leonardo.bootloader.name%=DriverInstall, USB\VID_2341&PID_0036
%leonardo.sketch.name%=DriverInstall, USB\VID_2341&PID_8036&MI_00
%lilypadUSB.bootloader.name%=DriverInstall, USB\VID_1B4F&PID_9207
%lilypadUSB.sketch.name%=DriverInstall, USB\VID_1B4F&PID_9208&MI_00
%mega2560rev3.name%=DriverInstall, USB\VID_2341&PID_0042
%mega2560.name%=DriverInstall, USB\VID_2341&PID_0010
%megaADK.name%=DriverInstall, USB\VID_2341&PID_003F
%megaADKrev3.name%=DriverInstall, USB\VID_2341&PID_0044
%micro.bootloader.name%=DriverInstall, USB\VID_2341&PID_0037
%micro.sketch.name%=DriverInstall, USB\VID_2341&PID_8037&MI_00
%mkr1000.sketch.name%=DriverInstall, USB\VID_2341&PID_804E&MI_00
%mkr1000.bootloader.name%=DriverInstall, USB\VID_2341&PID_004E
%uno.name%=DriverInstall, USB\VID_2341&PID_0001
%unoR3.name%=DriverInstall, USB\VID_2341&PID_0043
%usbserial.name%=DriverInstall, USB\VID_2341&PID_003B
%robotControl.bootloader.name%=DriverInstall, USB\VID_2341&PID_0038
%robotControl.sketch.name%=DriverInstall, USB\VID_2341&PID_8038&MI_00
%robotMotor.bootloader.name%=DriverInstall, USB\VID_2341&PID_0039
%robotMotor.sketch.name%=DriverInstall, USB\VID_2341&PID_8039&MI_00
%yun.bootloader.name%=DriverInstall, USB\VID_2341&PID_0041
%yun.sketch.name%=DriverInstall, USB\VID_2341&PID_8041&MI_00
%zero.edbg.name%=DriverInstall, USB\VID_03EB&PID_2157&MI_01
%zero.sketch.name%=DriverInstall, USB\VID_2341&PID_804D&MI_00
%zero.bootloader.name%=DriverInstall, USB\VID_2341&PID_004D
%sme_fox.sketch.name%=DriverInstall, USB\VID_2341&PID_E002&MI_00
%sme_fox.bootloader.name%=DriverInstall, USB\VID_2341&PID_E001

[DriverInstall]
include=mdmcpq.inf,usb.inf
CopyFiles = FakeModemCopyFileSection
AddReg=DriverAddReg

[DriverAddReg]
HKR,,DevLoader,,*ntkern 
HKR,,NTMPDriver,,usbser.sys 
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.Services]
include=mdmcpq.inf
AddService=usbser, 0x00000002, DriverService

[DriverService]
DisplayName=%ServiceName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys
LoadOrderGroup=Base

